# EPANET: Action Clauses

Action Clauses

An action clause in a Rule-Based Control takes the form of:

object id STATUS / SETTING IS value

where

object | = | LINK, PIPE, PUMP, or VALVE keyword
id | = | the object's ID label
value | = | a status condition (OPEN or CLOSED), pump speed setting, or valve setting

Some example action clauses are:
`LINK 23 STATUS IS CLOSED
PUMP P100 SETTING IS 1.5
VALVE 123 SETTING IS 90
`

See the notes for the [STATUS] section for conventions used in specifying link status and setting, particularly for control valves.